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	Technical Specifications

	

	Capacity
	Rectangular (h x w)
	Round
	Square

	90°
	14” x 14”
	14”
	14”

	

	Blade Size
	1 1/4” x 15’ 2”
	Remnant Length
	4.7” (11” w/OH bundling*)

	Blade Drive
	8.8 HP VFD
	Coolant Tank Capacity
	53 Gallons

	Machine Voltage
	480 v
	Machine Weight
	6,172 lbs.

	Blade Speed
	49-380 (50-660*) SFM
	Table Height
	34”

	Automatic Multi-indexing
	0-24”
	Dimensions (w x l x h)
	88” x 63” x 78”


	
**High blade speed option


	Standard Machine Features

	

	· Heavy-duty cast iron saw head
· Spilt front vise
· Cast iron shuttle features automatic multi-indexing up to 24” in a single stroke with automatic kerf compensation. Powered by ball screw and stepper motor.
· On-demand hydraulics save energy
· Steel guide arms mounted on linear rails. Hydraulically powered idler side guide arm is adjustable for proper spacing.
· 8.8 HP VFD. True direct blade drive – no belts/pulleys
	· Full capacity, full stroking hydraulic vises
· Hydraulic positive down feed 
· Blade chamber separates material from cut part 
· Cast iron band wheels
· Automatic PLC, touch screen control programmable up to 100 jobs with 20 in queue.
· Replaceable blade brush
· Robust steel base
· Automatic chip removal conveyor
· Easy access electrical panel and hydraulics
· Variable vise pressure 
	· Blade breakage switch
· Blade deviation monitor
· Designed for safety with saw-in-a-box style
· Out of stock switch 
· Electronic band tensioning with digital readout
· Replaceable carbide guide inserts
· Safety door interlocks
· Flood coolant with wash down hose
· Laser light
· Work light

	


	Optional Machine Features

	

	· Full capacity hydraulic overhead bundling*
· Mist lubrication
	· Power transformers
· Vertical rollers
	· Short remnant of 0.98”**
· Idler conveyors
· Powered conveyors

	*overhead bundling increases remnant length to 11” and reduces shuttle stroke to 21.5”
**cannot use option with overhead bundling

	
Additional Online Resources

	

	View additional resources such as feature descriptions, footprint drawings, images and videos on the HYDMECH web site at: https://www.hydmech.com/products/band-saws-horizontal-h-14a/ 


	Investment

	

	
	Part Number
	USD

	H-14A with standard productivity machine features
	16405000
	$54,500

	


	Step one – select options

	

	Full capacity hydraulic overhead bundling – two vises
	16405005
	$6,300

	Mist lubrication system (shop air required)
	16405060
	$1,900

	Power Transformer- change in house power from 480 v to 208 v
	-
	$1,700

	Power Transformer- change in house power from 480 v to 240 v
	-
	$1,700

	Power Transformer- change in house power from 480 v to 575 v
	-
	$1,700

	Short remnant – reduces remnant to 0.98”**
	16405065
	$4,900

	Vertical rollers – on machine
	16405025
	$1,800

	**cannot use option with overhead bundling


	Step two – select conveyors

HYDMECH designs and manufactures material handling systems for heavy-duty industrial applications.      We can build to your custom specifications or provide a turnkey engineered solution.

Note: All conveyor controls will be on a free-standing pedestal separate from the machine controls.

	

	Idler conveyors (26”W x 35”H)
	
	

	Type 2 - 5’ in feed/ out feed idler conveyor 
	18025261
	$4,700

	Type 2 - 10’ in feed/ out feed idler conveyor 
	18025262
	$8,900

	
	
	

	Powered conveyors (26”W x 35”H)
	
	

	Type 2 - 5’ in feed/ out feed powered conveyor 
	18020270
	$11,500

	Type 2 - 10’ in feed/ out feed powered conveyor 
	18020271
	$16,500

	Additional 10’ power add on section 
	18099788
	$11,500

	Pneumatic clutch 
	18092000
	$4,500

	
	
	

	Accessories for both idler and powered conveyors
	
	

	Filler plates – for 5’ conveyor
	18099091
	$1,900

	Filler plates – for 10’ conveyor
	18099092
	$3,800

	Coolant drip pan – for 5’ conveyor
	18099084
	$1,900

	Coolant drip pan – for 10’ conveyor
	18099083
	$3,800

	Vertical alignment roller 
	18099080
	$2,500

	Fork lift cut outs 
	18099095
	$2,500



	Terms

	

	Delivery:
	Contact factory
	Warranty:
	Two year parts, One year labor*

	F.O.B.:
	Conway, AR
	
	*Labor provided by dealer
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877-276-SAWS (7297) • www.hydmech.com • info@hydmech.com
HYDMECH reserves the right to modify this quotation without liability whatsoever. Specifications and pricing may change without prior notice.
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