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	Technical Specifications

	

	Capacity
	Rectangular (h x w)
	Round

	90°
	20” x 30”
	20”

	45°
	20” x 19”
	20” 

	30°
	20” x 12”
	14”

	

	Blade Size
	1 1/2” x 20’ 6”
	Work Load
	8,000 lbs.

	Blade Drive
	10 HP VFD
	Machine Weight
	7,700 lbs.

	Machine Voltage
	480 v
	Table Height
	32”

	Blade Speed
	50-350 SFM
	Dimensions (w x l x h)
	129” x 90” x 110”

	Coolant Tank Capacity
	9 Gallons
	
	




	Standard Machine Features

	

	· Automatic programmable mitering with “go to” angle functionality
· Automatic multi-indexing up to 33” in a single stroke. 
· Steel guide arms mounted on linear rails. Hydraulically powered idler side guide arm is adjustable for proper spacing.
· 10 HP VFD. True direct blade drive – no belts/pulleys
· Full capacity, full stroking hydraulic vises
· Hydraulic positive down feed 

	· Blade chamber separates material from cut part 
· Cast iron band wheels
· 8.5” color touch screen HMI. Mitsubishi FX5U PLC. No flipping from screen-to-screen, the control is interactive with messages for the operator that reduces the learning curve. User Friendly Graphical Icon programing for miter cutting, 1000 jobs, 20 jobs in queue
· Replaceable blade brush
· Robust steel base
· Automatic chip removal auger
	· Easy access electrical panel and hydraulics Blade breakage switch
· Hardened replaceable wear plates on material vises
· Hydraulic band tensioning
· Hydraulic carbide guide tensioning
· Safety door interlocks
· Flood coolant with wash down hose
· Laser light
· Work light
· Out of stock switch
· Variable vise pressure 

	


	Optional Machine Features

	

	· Blade deviation
· Full capacity hydraulic overhead bundling
· Chip bucket
	· Mist lubrication
· Remote console - 10’ cord
· Outboard vise clamping options available upon request
	· Power transformer
· Vertical rollers
· Idler conveyors
· Powered conveyors


	

	Additional Online Resources

	

	View additional resources such as feature descriptions, footprint drawings, images and videos on the HYDMECH web site at: https://www.hydmech.com/products/band-saws-horizontal-pivot-m-20a/ 


	Investment

	

	
	Part Number
	USD

	M-20A with standard productivity machine features
	1203000
	$86,500

	

	Step one – select options

	

	Chip bucket
	14020030
	$700

	Full capacity hydraulic overhead bundling – two vises
	12010010
	$6,500

	Mist lubrication system (shop air required)
	12030060
	$1,900

	Power Transformer- change in house power from 480 v to 208 v
	-
	$1,700

	Power Transformer- change in house power from 480 v to 240 v
	-
	$1,700

	Power Transformer- change in house power from 480 v to 575 v
	-
	$1,700

	Remote console – 10’ cord
	12030780
	$5,500

	Vertical rollers – on machine base
	12010025
	$1,800

	Blade deviation monitor
	12030030
	$4,500

	

	Step two – select conveyors

HYDMECH designs and manufactures material handling systems for heavy-duty industrial applications.      We can build to your custom specifications or provide a turnkey engineered solution.

Note: All conveyor controls will be on a free-standing pedestal separate from the machine controls.

	

	Idler conveyors (36”W x 32”H)
	
	

	Type 2 -  5’ in feed/ out feed idler conveyor 
	18020361
	$5,200

	Type 2 -  10’ in feed/ out feed idler conveyor 
	18020362
	$9,900

	
	
	

	Powered conveyors (36”W x 32”H)
	
	

	Type 2 -  5’ in feed/ out feed powered conveyor 
	18020363
	$10,500

	Type 2 -  10’ in feed/ out feed powered conveyor 
	18020364
	$17,500

	Additional 10’ power add on section 
	18099784
	$12,500

	Pneumatic clutch 
	18092000
	$4,500

	
	
	

	Accessories for both idler and powered conveyors
	
	

	Filler plates – for 5’ conveyor
	18099091
	$1,900

	Filler plates – for 10’ conveyor
	18099092
	$3,800

	Coolant drip pan – for 5’ conveyor
	18099084
	$1,900

	Coolant drip pan – for 10’ conveyor
	18099083
	$3,800

	Vertical alignment roller 
	18099080
	$2,500

	Fork lift cut outs 
	18099095
	$2,500


	Terms

	

	Delivery:
	Contact factory
	Warranty:
	Two year parts, One year labor*

	F.O.B.:
	Woodstock, ON
	
	*Labor provided by dealer
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FOUNDATION PLAN
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SPECIFICATIONS

CAPACITY

BLADE

BLADE DRIVE
HYDRAULIC DRIVE
MACHINE WEIGHT

20" DIA
30" x 20"

11/2x206"
10 HP

3HP
7100 LBS
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